# Routes and streets

Metadata also available as - [Parseable text]

# Metadata:

- Identification_Information
- Data_Quality_Information
- Spatial_Data_Organization_Information
- Spatial_Reference_Information
- Entity_and_Attribute_Information
- Distribution_Information
- Metadata_Reference_Information
- Lineage

Identification_Information:
  Citation:
    Citation_Information:
      Originator: Bureau of Stattistics and Plans, Government of Guam
      Publication_Date: May 2013
      Title: Routes and streets
      Geospatial_Data_Presentation_Form: vector digital data
      Edition: Partial Update of 1st Edition
      Publication_Information:
        Publication_Place: Bureau of Statistics and Plans
  Description:
    Abstract:
      This is the streets data layer for the island of Guam. This dataset has been updated in 2012/2013. The update was mainly based on the WorldView2 2011 imagery and a draft parcel layer (for right-of-way vs. driveway clarification). Name changes have not been adressed in this update, nor geocoding information. Also, this update is by no means complete but should incorporate major changes in the road network reflected in the 2011 imagery.
    Purpose:
      The data layer was created to provide an up-to-date streets layer for government operations, private sector and public use.
    Supplemental_Information: The streets layer has been updated in 2012/2013.
  Time_Period_of_Content:
    Time_Period_Information:
      Single_Date/Time:
        Calendar_Date: May 2013
        Time_of_Day: 9am
    Currentness_Reference: ground condition
  Status:
    Progress: In work
    Maintenance_and_Update_Frequency: Continually
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: 144.620249
      East_Bounding_Coordinate: 144.948392
      North_Bounding_Coordinate: 13.652449
      South_Bounding_Coordinate: 13.246765
  Keywords:
    Theme:
      Theme_Keyword_Thesaurus: path
      Theme_Keyword: transportation
      Theme_Keyword: streets
      Theme_Keyword: roads
      Theme_Keyword: routes
      Theme_Keyword: highways
    Theme:
      Theme_Keyword_Thesaurus: conveyance
      Theme_Keyword: transport
      Theme_Keyword: streets
    Theme:
      Theme_Keyword: transportation
      Theme_Keyword: streets
      Theme_Keyword: highways
      Theme_Keyword: roads
    Place:
      Place_Keyword: Pacific Islands
      Place_Keyword: Guam
      Place_Keyword: Micronesia
      Place_Keyword: Western Pacific
      Place_Keyword: Northwestern Pacific
      Place_Keyword: United States Possesion
  Access_Constraints:
    For planning purposes only! Though efforts were made to obtain accurate and timely data the Bureau assumes no liability for any inaccuracies in this product. Additionally, names may have changed and new streets built since the production of this product.
  Use_Constraints:
    Data set is not for use in litigation. Bureau of Statistics & Plans (BSP) cannot assume liability for any damages or misrepresentations caused by any inaccuracies in the data or as a result of the data to be in a particular system.The Burea should be given credit for the work involved in creating the dataset.
  Point_of_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: Vange Lujan
        Contact_Organization: Bureau of Statistics & Plans (BSP)
      Contact_Position: Guam Coastal Management Adminstrator/ Acting GIS Manager
      Contact_Address:
        Address_Type: mailing and physical address
        Address: P.O. Box 2950
        City: Hagatna
        State_or_Province: Guam
        Postal_Code: 96932
        Country: USA
        Address: 513 W Marine Corps Dr
      Contact_Voice_Telephone: 671-472-4201-3
      Contact_Facsimile_Telephone: 671-477-1812
      Contact_Electronic_Mail_Address: vange.lujan@bsp.guam.gov
      Hours_of_Service: 8am - 5pm Chamorro Time (+10 UTC)
  Data_Set_Credit:
    The layer was created by the Bureau of Statistics & Plans (BSP) Land Use Planning/Coastal Management Program. The department of Public Works Office of Highway Planning assisted. The Mayors Council provided assistance by providing feedback of streets names in their village.
  Security_Information:
    Security_Classification: Unclassified
  Native_Data_Set_Environment:
    Microsoft Windows XP Version 5.1 (Build 2600) Service Pack 3; ESRI ArcCatalog 9.3.1.4000

Data_Quality_Information:
  Attribute_Accuracy:
    Attribute_Accuracy_Report:
      Street names were obtained from 3 different sources. Dept of Public Works Office of Highway Planning maps, the Bureaus'existing streets layer and the municipal mayors. The municipal Mayors became the final authority on the accuracy of the names. The process of obtaining names was an iterative one with an ititial, draft and final draft document given to the Mayors for review. For the most part most Mayors responded to the draft stage. A small percentage of Mayors hesitated to rename temporarily named (S1, S2) streets due to the legal process to naming a street not being completed at the time of this collections process.
  Logical_Consistency_Report:
    Data are believed to be logically consistent. Topology was cleaned utilizing the ESRI clean topology tool.
  Completeness_Report:
    Presently the geocoding of streets to range of structures/building address numbers is awaiting the update of house numbers in that update project. All streets on Guam, including those on Military Reservations are in the layer.
  Positional_Accuracy:
    Horizontal_Positional_Accuracy:
      Horizontal_Positional_Accuracy_Report:
        The streets layer was created by updating the existing streets layer in Guam Grid 1963 Projection. This was converted to Guam Grid 1993 Projection. The resulting layer needed to be spatially adjusted to line up better. Cross cross checks with the Guam Geodetic Network survey marks database, land parcels layer with associated Rights-of-Ways corridors, High Accuracy Reference Network (HARN) benchmarks and Digital Globe satellite Imagery. The GGN and land parcels the most survey accurate cross checks. Most GGN survey marks are within 1-5 meters from the sides of streets. Parcels are also based on survey data. Not all streets overlayed their locations on the imagery used though the accuracy of the imagery itself may be in question. Therefore the survey level features cited above ensured closer alignment to what are real worl coordinates.
    Vertical_Positional_Accuracy:
      Vertical_Positional_Accuracy_Report:
        The vertical accuracy of the layer was not verified at this time. There are however vertical benchmarks that circle the island on the major routes that were established in late 2005. The data can be obtained form the U.S. National Geodetic Survey website under Guam.
  Lineage:
    Process_Step:
      Process_Description:
        This layer was created by the Bureau of Statistics & Plans (BSP) Land Use Planning/Coastal Management Program. The Department of Public Works Office of Highway Planning assisted. The Mayors Council provided assistance by providing feedback of streets names in their village. Street names were obtained from 3 different sources. Dept of Public Works Office of Highway Planning maps, the Bureau existing streets layer and the municipal mayors. The original Bureau data was converted from Guam Grid 1963 projection to Guam Grid 1993. It did not line up on the imagery accurately in some areas. Survey points were utilized to asses the relative accuracy of the data layer.
      Process_Date: Januray 2006 - October 2006
      Process_Contact:
        Contact_Information:
          Contact_Person_Primary:
            Contact_Person: Vange Lujan
            Contact_Organization: Bureau of Statistics & Plans
          Contact_Position: Guam Coastal Management Adminstrator/ Acting GIS Manager
          Contact_Address:
            Address_Type: mailing and physical address
            Address: POB 3643
            Address: 513 W Marine Corps Dr.
            City: Hagatna
            State_or_Province: Guam
            Postal_Code: 96932 or 96910
          Contact_Voice_Telephone: 671-472-4201-3/475-9665
          Contact_Facsimile_Telephone: 671-477-1812
          Contact_Electronic_Mail_Address: vange.lujan@bsp.guam.gov
          Hours_of_Service: 8am - 5pm Chamorro time (+10 UTC)
    Process_Step:
      Process_Description:
        The recent update was mainly based on the WorldView2 2011 imagery and a draft parcel layer (for right-of-way vs. driveway clarification). Name changes have not been adressed in this update, nor geocoding information. Also, this update is by no means complete but should incorporate major changes in the road network reflected in the 2011 imagery.
      Time_of_Day: 17344300
      Process_Contact:
        Contact_Information:
          Contact_Person_Primary:
            Contact_Person: Maria Kottermair
            Contact_Organization: Guam Coastal Management Plan, Bureau of Statistics and Plans
          Contact_Position: GIS support for GCMP, University of Guam (WERI)
          Contact_Electronic_Mail_Address: mariakottermair@uguamlive.uog.edu
      Process_Date: 2012-2013

Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method: Vector
  Point_and_Vector_Object_Information:

Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Planar:
      Planar_Coordinate_Information:
        Planar_Coordinate_Encoding_Method: coordinate pair
        Planar_Distance_Units: meters
    Geodetic_Model:
      Horizontal_Datum_Name: D_WGS_1984
      Ellipsoid_Name: WGS_1984
  Vertical_Coordinate_System_Definition:
    Altitude_System_Definition:
      Altitude_Resolution: 0.000001
      Altitude_Encoding_Method:
        Explicit elevation coordinate included with horizontal coordinates

Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: streets
    Attribute:
      Attribute_Label: OBJECTID
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: Esri
      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: OBJECTID_1
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Shape
      Attribute_Definition: Feature geometry.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Coordinates defining the features.
    Attribute:
      Attribute_Label: TAG
      Attribute_Definition: Name used to identify the feature for labeling purposes
      Attribute_Domain_Values:
        Unrepresentable_Domain: Coordinates defining the features.
    Attribute:
      Attribute_Label: PRE_DIR
      Attribute_Definition: direction of street, eg. E or W
    Attribute:
      Attribute_Label: PRE_TYPE
      Attribute_Definition: used to denote Routes and other special street types
    Attribute:
      Attribute_Label: STREETNAME
      Attribute_Definition: name of street
      Attribute_Domain_Values:
        Unrepresentable_Domain: Coordinates defining the features.
    Attribute:
      Attribute_Label: STR_TYPE
      Attribute_Definition: type of street, eg. lane, avenue
    Attribute:
      Attribute_Label: LTOLFROM
      Attribute_Definition: left to left from for geocoding
    Attribute:
      Attribute_Label: CSTATUS
    Attribute:
      Attribute_Label: LFROM
      Attribute_Definition: left from
    Attribute:
      Attribute_Label: LTO
      Attribute_Definition: left to
    Attribute:
      Attribute_Label: RFROM
      Attribute_Definition: right from
    Attribute:
      Attribute_Label: RTO
      Attribute_Definition: right to
    Attribute:
      Attribute_Label: O_SNAME
    Attribute:
      Attribute_Label: VILLAGE
      Attribute_Definition: village street located in
    Attribute:
      Attribute_Label: NO_LANES
    Attribute:
      Attribute_Label: Length_mtr
    Attribute:
      Attribute_Label: Shape_Length
      Attribute_Definition: Length of feature in internal units.
      Attribute_Definition_Source: Esri
      Attribute_Domain_Values:
        Unrepresentable_Domain: Positive real numbers that are automatically generated.
  Overview_Description:
    Entity_and_Attribute_Overview:
      The tag is the street name for labeling purposes. So if a route it may only include the route number. In addition Chamorro language prefixes of Chalan (street) or Kayon or Kayen (trail) describe the type of street somewhat. It is usually a name given by the Mayors but not at this time being assigned to features in the convention of their description.

Distribution_Information:
  Distributor:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: Bureau of Statistics & Plans (BSP)
        Contact_Person: Vange Lujan
      Contact_Position: Guam Coastal Management Adminstrator/ Acting GIS Manager
      Contact_Address:
        Address_Type: mailing address
        Address: P.O. Box 2950
        City: Hagatna
        State_or_Province: Guam
        Postal_Code: 96932
        Country: United States
      Contact_Voice_Telephone: 671-472-4201-3
      Contact_Facsimile_Telephone: 671-477-1812
      Contact_Electronic_Mail_Address: vange.lujan@bsp.guam.gov
      Hours_of_Service: 8am-5pm
  Resource_Description:
    Downloadable Data but not presently available on the internet so it must be obtained from the Bureau directly.
  Distribution_Liability:
    Users must assume responsibility to determine the appropriate use for this data.
  Standard_Order_Process:
    Ordering_Instructions: Please ID Point of Contact indicated
    Digital_Form:
      Digital_Transfer_Information:
        Format_Name: geodatabase
        Format_Version_Number: 9x
        Transfer_Size: 184 megabytes
    Fees: None at this time
    Turnaround: 2 weeks

Metadata_Reference_Information:
  Metadata_Date: 20130828
  Metadata_Future_Review_Date: At next update of data layer
  Metadata_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Organization: Guam Coastal Management Plan, Bureau of Statistics and Plans
        Contact_Person: Maria Kottermair
      Contact_Position: GIS support for GCMP, University of Guam (WERI)
      Contact_Address:
        Address_Type: mailing and physical address
        City: Hagatna
        State_or_Province: Guam
        Postal_Code: 96932 or 96910 (physical)
        Address: POB 2950
        Address: 513 W Marine Corps Dr
        Country: USA
      Contact_Facsimile_Telephone: 671-477-1812
      Contact_Electronic_Mail_Address: mariakottermair@uguamlive.uog.edu
      Hours_of_Service: 8am - 5 pm local Guam Time
  Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Metadata_Access_Constraints: None
  Metadata_Use_Constraints: None

Lineage:

Generated by `mp` version 2.9.3 on Sun Oct 20 21:33:57 2013