# USGS Topo Map (DRGs)

Metadata also available as - [Parseable text]

# Metadata:

- Identification_Information
- Data_Quality_Information
- Spatial_Data_Organization_Information
- Spatial_Reference_Information
- Entity_and_Attribute_Information
- Distribution_Information
- Metadata_Reference_Information

Identification_Information:
  Citation:
    Citation_Information:
      Title: USGS Topo Map (DRGs)
      Geospatial_Data_Presentation_Form: raster digital data
  Description:
    Abstract:
      This layer shows the USGS topographic map of Guam. This image is a composite image, comprised of all nine 7.5-minute quadrangle maps that cover the island of Guam. The raster layer was clipped to the shoreline of Guam.
    Purpose:
      To provide a single image file that shows the USGS topographic map.
  Time_Period_of_Content:
    Time_Period_Information:
      Single_Date/Time:
        Calendar_Date: 2002
    Currentness_Reference: ground condition
  Status:
    Progress: Complete
    Maintenance_and_Update_Frequency: As needed
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: 144.616019
      East_Bounding_Coordinate: 144.959891
      North_Bounding_Coordinate: 13.655217
      South_Bounding_Coordinate: 13.242228
  Keywords:
    Theme:
      Theme_Keyword: topography
      Theme_Keyword: USGS
      Theme_Keyword: topographic map
      Theme_Keyword: 7.5-minute quadrangles
      Theme_Keyword: DRGs
      Theme_Keyword: digital raster graphics
    Place:
      Place_Keyword: Guam
      Place_Keyword: Pacific Ocean
      Place_Keyword: Philippine Sea
    Stratum:
    Temporal:
  Point_of_Contact:
    Contact_Information:
      Contact_Position: GIS Manager
      Hours_of_Service: 1400 - 1600 Hawaii Time
      Contact_Organization_Primary:
        Contact_Organization: Guam Coastal Management Program, Bureau of Statistics and Plans
  Data_Set_Credit:
    Original maps by USGS. Composite raster image created by Guam Coastal Management Program, Bureau of Statistics and Plans.
  Native_Data_Set_Environment:
    Microsoft Windows XP Version 5.1 (Build 2600) Service Pack 2; ESRI ArcCatalog 9.2.4.1420

Data_Quality_Information:
  Logical_Consistency_Report: See USGS website on information about the DRGs
  Lineage:
    Process_Step:
      Process_Description:
        Created map document with all nine USGS topo quadrangle maps. Exported as tiff with worldfile. Clip raster to shoreline.
      Process_Date: 2013
      Process_Contact:
        Contact_Information:
          Contact_Person_Primary:
            Contact_Person: Maria Kottermair
            Contact_Organization:
              Guam Coastal Management Program (GCMP), Bureau of Statistics and Plans
          Contact_Position: GIS Support for GCMP, University of Guam (WERI)
          Contact_Electronic_Mail_Address: mariakottermair@uguamlive.uog.edu
    Source_Information:
      Source_Citation:
        Citation_Information:
          Title: USGS 7.5-minute quadrangle maps for Guam (DRGs)
          Originator: U.S. Geological Survey
          Geospatial_Data_Presentation_Form: raster digital data
          Other_Citation_Details: Nine quadrangle maps for Guam

Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method: Raster
  Point_and_Vector_Object_Information:
    SDTS_Terms_Description:
      SDTS_Point_and_Vector_Object_Type: String
      Point_and_Vector_Object_Count: 294194

Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Planar:
      Planar_Coordinate_Information:
        Planar_Coordinate_Encoding_Method: row and column
        Coordinate_Representation:
          Abscissa_Resolution: 4.000000
          Ordinate_Resolution: 4.000000
        Planar_Distance_Units: meters
    Geodetic_Model:
      Horizontal_Datum_Name: D_WGS_1984
      Ellipsoid_Name: WGS_1984
  Vertical_Coordinate_System_Definition:
    Altitude_System_Definition:
      Altitude_Resolution: 0.000100
      Altitude_Encoding_Method:
        Explicit elevation coordinate included with horizontal coordinates

Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: usgs_topo_quadrangles
    Attribute:
      Attribute_Label: OID
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: Esri
      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Value
    Attribute:
      Attribute_Label: Count

Distribution_Information:
  Distributor:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: Mr. Victor Torres
        Contact_Organization: Government of Guam, Bureau of Statistics and Plans
      Contact_Position: GIS Manager
      Contact_Address:
        Address: P.O. Box 2950
        City: Hagatna
        State_or_Province: Guam
        Postal_Code: 96932
      Contact_Voice_Telephone: (671) 472-4201
  Resource_Description: Downloadable Data
  Distribution_Liability:
    Consult with Government of Guam, Bureau of Plans and Statistics.
  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Transfer_Size: 1597.707

Metadata_Reference_Information:
  Metadata_Date: 20130906
  Metadata_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: Guam Coastal Management Program, Bureau of Statistics and Plans
  Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Metadata_Access_Constraints: None
  Metadata_Use_Constraints: None
  Metadata_Security_Information:
    Metadata_Security_Classification: Unclassified

Generated by `mp` version 2.9.3 on Sun Oct 20 21:41:03 2013